{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":78,"n_cols":4,"rows_kept":78,"flags":["formulas_cached_only"]}
["点名","点值","描述","标识(1:标识总貌图页面配置点)"]
["YMG110kVAmx1A90","HB_GD_DXF_DQ_P1_L1_001_DI0402","[110kV测控]1A90合位"]
["YMG110kVAmx1A9","HB_GD_DXF_DQ_P1_L1_001_DI0397","[110kV测控]1A9合位"]
["YMG110kVAmx1A10","HB_GD_DXF_DQ_P1_L1_001_DI0400","[110kV测控]1A10合位"]
["YMG110kVAmx111-X0","HB_GD_DXF_DQ_P1_L1_001_DI0370","[110kV测控]111-线0合位"]
["YMG110kVAmx111-A0","HB_GD_DXF_DQ_P1_L1_001_DI0363","[110kV测控]111-A0合位"]
["YMG110kVAmx111-1","HB_GD_DXF_DQ_P1_L1_001_DI0365","[110kV测控]111-1合位"]
["YMG110kVAmx111","HB_GD_DXF_DQ_P1_L1_001_DI0357","[110kV测控]111断路器合位",1]
["YMG110kVAmx111-A","HB_GD_DXF_DQ_P1_L1_001_DI0360","[110kV测控]111-A合位"]
["YMG110kVAmx111-10","HB_GD_DXF_DQ_P1_L1_001_DI0368","[110kV测控]111-10合位"]
["YMG110kVAmx101-A","HB_GD_DXF_DQ_P1_L1_001_DI0476","[主变高压侧测控]101-A合位"]
["YMG110kVAmx101-A0","HB_GD_DXF_DQ_P1_L1_001_DI0479","[主变高压侧测控]101-A0合位"]
["XC66kVC1629D14","HB_GD_DXF_DQ_P1_L1_001_DI0481","[主变高压侧测控]101-1合位"]
["YMG110kVAmx101","HB_GD_DXF_DQ_P1_L1_001_DI0473","[主变高压侧测控]101断路器合位",1]
["YMG1Zb101-A0","HB_GD_DXF_DQ_P1_L1_001_DI0479","[主变高压侧测控]101-A0合位"]
["YMG1Zb101-B0","HB_GD_DXF_DQ_P1_L1_001_DI0486","[主变高压侧测控]101-变0合位"]
["YMG1Zb1010","HB_GD_DXF_DQ_P1_L1_001_DI0488","[主变高压侧测控]1010合位"]
["YMG1Zb301","HB_GD_DXF_DQ_P1_L1_001_DI0537","[主变低压侧测控]301断路器合位",1]
["YMG1Zb301sc","HB_GD_DXF_DQ_P1_L1_001_DI0540","[主变低压侧测控]301手车工作位置",1]
["YMG0-4kVmx313-x0","HB_GD_DXF_DQ_P1_L1_001_DI0337","[站用变保护]313-线0合位"]
["YMG0-4kVmx1DK","HB_GD_DXF_DQ_P1_L1_001_DI0333","[站用变保护]断路器位置"]
["YMG04kVmx313","HB_GD_DXF_DQ_P1_L1_001_DI0334","[站用变保护]313断路器合位"]
["YMG04kVmx313sc","HB_GD_DXF_DQ_P1_L1_001_DI0343","[站用变保护]313手车工作位置"]
["YMG35kVJdIx311","HB_GD_DXF_DQ_P1_L1_001_DI0048","[集电I线保护]311断路器合位",1]
["YMG35kVJdIx311sc","HB_GD_DXF_DQ_P1_L1_001_DI0057","[集电I线保护]311手车工作位置",1]
["YMG35kVJdIx311-x0","HB_GD_DXF_DQ_P1_L1_001_DI0051","[集电I线保护]311-线0合位"]
["YMG35kVJdIIx312","HB_GD_DXF_DQ_P1_L1_001_DI0117","[集电II线保护]312断路器合位",1]
["YMG35kVJdIIx312sc","HB_GD_DXF_DQ_P1_L1_001_DI0126","[集电II线保护]312手车工作位置",1]
["YMG35kVJdIIx312-x0","HB_GD_DXF_DQ_P1_L1_001_DI0120","[集电II线保护]312-线0合位"]
["YMG35kVDrq314","HB_GD_DXF_DQ_P1_L1_001_DI0186","[一组电容器保护]314断路器合位"]
["YMG35kVDrq314sc","HB_GD_DXF_DQ_P1_L1_001_DI0199","[一组电容器保护]314手车工作位置"]
["XC66kVC1629D8","HB_GD_DXF_DQ_P1_L1_001_DI0200","[一组电容器保护]314-线00合位"]
["YMG35kVDrq314-1","HB_GD_DXF_DQ_P1_L1_001_DI0195","[一组电容器保护]314-1分支隔离刀合位"]
["YMG35kVDrq314-x0","HB_GD_DXF_DQ_P1_L1_001_DI0189","[一组电容器保护]314-线0合位"]
["YMG35kVSvg315","HB_GD_DXF_DQ_P1_L1_001_DI0261","[SVG保护]315断路器合位"]
["YMG35kVSvg315sc","HB_GD_DXF_DQ_P1_L1_001_DI0273","[SVG保护]315手车工作位置"]
["YMG35kVSvg315-1","HB_GD_DXF_DQ_P1_L1_001_DI0269","[SVG保护]315-1合位"]
["XC66kVC1629D6","HB_GD_DXF_DQ_P1_L1_001_DI0274","[SVG保护]315-线00合位"]
["YMG35kVSvg315-x0","HB_GD_DXF_DQ_P1_L1_001_DI0263","[SVG保护]315-线0合位"]
["YMG110KVckia","HB_GD_DXF_DQ_P1_L1_001_AI0174","[110kV测控]ia"]
["YMG110KVckq","HB_GD_DXF_DQ_P1_L1_001_AI0178","[110kV测控]q"]
["YMG110KVckp","HB_GD_DXF_DQ_P1_L1_001_AI0177","[110kV测控]p"]
["YMG110KVckcos","HB_GD_DXF_DQ_P1_L1_001_AI0179","[110kV测控]cos"]
["YMG110KVckux","HB_GD_DXF_DQ_P1_L1_001_AI0170","[110kV测控]ux"]
["YMG110KVckua","HB_GD_DXF_DQ_P1_L1_001_AI0180","[公用测控]110kV母线电压u1a"]
["YMG110KVckub","HB_GD_DXF_DQ_P1_L1_001_AI0181","[公用测控]110kV母线电压u1b"]
["YMG110KVckuc","HB_GD_DXF_DQ_P1_L1_001_AI0182","[公用测控]110kV母线电压u1c"]
["YMG110KVckuab","HB_GD_DXF_DQ_P1_L1_001_AI0183","[公用测控]110kV母线电压u1ab"]
["YMG110KVckubc","HB_GD_DXF_DQ_P1_L1_001_AI0184","[公用测控]110kV母线电压u1cb"]
["YMG110KVckuca","HB_GD_DXF_DQ_P1_L1_001_AI0185","[公用测控]110kV母线电压u1ca"]
["YMG110KVck3u0","HB_GD_DXF_DQ_P1_L1_001_AI0186","[公用测控]110kV母线电压3U0"]
["YMG1Zybia","HB_GD_DXF_DQ_P1_L1_001_AI0156","[站用变保护]A相电流"]
["YMG1Zybq","HB_GD_DXF_DQ_P1_L1_001_AI0165","[站用变保护]无功功率"]
["YMG1Zybcos","HB_GD_DXF_DQ_P1_L1_001_AI0166","[站用变保护]功率因素"]
["YMG1Zybp","HB_GD_DXF_DQ_P1_L1_001_AI0164","[站用变保护]有功功率"]
["YMG35KVmxua","HB_GD_DXF_DQ_P1_L1_001_AI0187","[公用测控]35kV母线电压u2a"]
["YMG35KVmxub","HB_GD_DXF_DQ_P1_L1_001_AI0188","[公用测控]35kV母线电压u2b"]
["YMG35KVmxuc","HB_GD_DXF_DQ_P1_L1_001_AI0189","[公用测控]35kV母线电压u2c"]
["YMG35KVmxuab","HB_GD_DXF_DQ_P1_L1_001_AI0190","[公用测控]35kV母线电压u2ab"]
["YMG35KVmxucb","HB_GD_DXF_DQ_P1_L1_001_AI0191","[公用测控]35kV母线电压u2cb"]
["YMG35KVmxuca","HB_GD_DXF_DQ_P1_L1_001_AI0192","[公用测控]35kV母线电压u2ca"]
["YMG35KVm3u0","HB_GD_DXF_DQ_P1_L1_001_AI0193","[公用测控]35kV母线电压3U0"]
["YMGJdIxia","HB_GD_DXF_DQ_P1_L1_001_AI0115","[集电I线保护]A相电流"]
["YMGJdIxp","HB_GD_DXF_DQ_P1_L1_001_AI0123","[集电I线保护]有功功率"]
["YMGJdIxq","HB_GD_DXF_DQ_P1_L1_001_AI0124","[集电I线保护]无功功率"]
["YMGJdIIxia","HB_GD_DXF_DQ_P1_L1_001_AI0126","[集电I线保护]A相电流"]
["YMGJdIIxp","HB_GD_DXF_DQ_P1_L1_001_AI0134","[集电II线保护]有功功率"]
["YMGJdIIxq","HB_GD_DXF_DQ_P1_L1_001_AI0135","[集电II线保护]无功功率"]
["YMGDrqia","HB_GD_DXF_DQ_P1_L1_001_AI0137","[一组电容器保护]A相电流"]
["YMGDrqp","HB_GD_DXF_DQ_P1_L1_001_AI0145","[一组电容器保护]有功功率"]
["YMGDrqq","HB_GD_DXF_DQ_P1_L1_001_AI0146","[一组电容器保护]无功功率"]
["YMGSvgia","HB_GD_DXF_DQ_P1_L1_001_AI0148","[SVG保护]A相电流"]
["YMGSvgp","HB_GD_DXF_DQ_P1_L1_001_AI0153","[SVG保护]有功功率"]
["YMGSvgq","HB_GD_DXF_DQ_P1_L1_001_AI0154","[SVG保护]无功功率"]
["YMG35KVZRZWD","HB_GD_DXF_DQ_P1_L1_001_AI0221","[复合信号虚装置]主变绕组温度"]
["YMG35KVZYW1","HB_GD_DXF_DQ_P1_L1_001_AI0219","[复合信号虚装置]主变油温1"]
["YMG35KVZYW2","HB_GD_DXF_DQ_P1_L1_001_AI0220","[复合信号虚装置]主变油温2"]
["YMG35KVDW","HB_GD_DXF_DQ_P1_L1_001_AI0218","[复合信号虚装置]变压器档位"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}